CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.0/conf/instr/spect/uxnmr.info
Date         : Wed Dec  5 10:23:11 2018
Release      : TopSpin 3.6.0
Installed in : /opt/topspin3.6.0
Host         : av700hd
OS           : CentOS Linux release 7.5.1804 (Core) 
CPU          : Intel(R) Xeon(R) CPU E5-1620 v3 @ 3.50GHz (8 cores at 1280 MHz with Hyperthreading)
User         : schwalbe
System       : Avance III HD 700 NMR spectrometer
1H-frequency : 700.17 MHz
Description  : AV700HD+CRPQCI5mm
Location     : UNI Frankfurt
Bruker Order : 10196848
Configured in: av700hd:/opt/topspin3.6.0/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 5
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/04862 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.3 REC-1  AQS RXAD/2 1000 Z130589/401 ECL 00.03
     3   0x34 0xda   0x1        X  2.3 REF-1  
     4   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00590 ECL 01.03 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00591 ECL 01.03 FPGA-Vs=20131031
     6   0x28 0x33     0        S  1.3 SGU-3  AQS SGU/3 1200 (2CH) Z117130/00593 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  2.0 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0857 W1345093/0857 ECL 12:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0857 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/5220 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010900 ECL 50
BLA_W1345093_0862 W1345093/0862 ECL 12:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0862 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/5219 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010932 ECL 50
BLA_W1345097_0378 W1345097/0378 ECL 20:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0378 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/5209 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010902 ECL 50
LTRX Z109891/00334 ECL 02.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00334 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20170712
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 700: Z109891/00334 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/02956 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/03295 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.90:/dev/tty04

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.8%/0.2deg, reflection meter)
                PN=Z103206, SN=00347 from 20150824
    Module  2 : 2H
                PN=Z003474, SN=00440 from 20150817
    Module  3 : XBB19F 2HS
                PN=Z003507, SN=00976 from 20150810
    Module  4 : XBB19F 2HS
                PN=Z003507, SN=00977 from 20150810
    Module  5 : 31P
                PN=Z102450, SN=00208 from 20150323
    Module  6 : 13C
                PN=Z003525, SN=00334 from 20150616
    Module  7 : 15N
                PN=Z003531, SN=00330 from 20150417



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 700 W1345097/0378 at TCP/IP 149.236.99.91)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0862 at TCP/IP 149.236.99.92)
SGU2 NORM output -> input 2 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 700 W1345097/0378 at TCP/IP 149.236.99.91)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0862 at TCP/IP 149.236.99.92)
SGU3 AUX  output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0857 at TCP/IP 149.236.99.93)
SGU4 NORM output -> input 3 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0862 at TCP/IP 149.236.99.92)
SGU4 AUX  output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0857 at TCP/IP 149.236.99.93)
SGU5 NORM output -> input 3 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 700 W1345097/0378 at TCP/IP 149.236.99.91)
SGU5 AUX  output -> input 4 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 700 W1345097/0378 at TCP/IP 149.236.99.91)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0857 at TCP/IP 149.236.99.93:
- amplifier X-500W uses blanking 5

transmitter 2 = BLAX500 E 6-365MHZ INR W1345093/0862 at TCP/IP 149.236.99.92:
- amplifier X-500W uses blanking 4

transmitter 3 = BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 700 W1345097/0378 at TCP/IP 149.236.99.91:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W uses blanking 7

transmitter 4 = BSMS/2 LOCK TRANSCEIVER 700 Z109891/00334 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


